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[bookmark: Xf1ba02bdc5918098f86f24156312d93acfd671a]Slides 5.11: Build the Drawstring Bag, and the Stitch Sampler Check
Slide outline for Lesson 5.11, three days, eighteen slides. Slides 1 to 7 are Day 1 (cut, mark, pin, first seam). Slides 8 to 12 are Day 2 (second seam, the channel, the sampler scrap). Slides 13 to 18 are Day 3 (turn, cord, finish, and the check). The hand path is named on every work slide so the hand station never waits for an instruction.
[bookmark: slide-1-day-1-the-build]Slide 1 (Day 1): The build
· Lesson 5.11, day one of three
· A drawstring bag: cut to a pattern, machine seams, turned right side out, a channel, a cord
· Hand station: the felt pouch, hand backstitched, same checklist, same rubric
· Machines are threaded. I did it this morning. Today we sew. Image: a finished drawstring bag, closed, next to a finished felt pouch.
[bookmark: slide-2-do-now]Slide 2: Do now
· What will you put in your bag?
· Write the order: cut, mark, pin, sew
· What happens if you swap the first two? Image: the bag pattern from Handout 05.11.
[bookmark: slide-3-three-things-wrong-with-this-one]Slide 3: Three things wrong with this one
· Pass the bad bag around
· Write down three things wrong with it
· Your checklist today is exactly that list Image: the deliberately bad bag: wandering seam, unlocked seam end, channel sewn shut at one end.
[bookmark: slide-4-the-pattern-one-more-time]Slide 4: The pattern, one more time
· The seam allowance is a quarter inch; the needle plate has a guide line for it
· Right sides TOGETHER, inside out, because this bag gets turned
· The side seams STOP at the channel marks. The gap is not a mistake, it is the door the cord comes through. Image: the pattern with the fold line, seam lines, and the shaded channel area labeled LEAVE OPEN HERE.
[bookmark: slide-5-pins-and-machines]Slide 5: Pins and machines
· Pins perpendicular to the seam, heads out
· Every pin comes OUT before it reaches the foot
· You never sew over a pin: a needle that hits a pin breaks
· And a broken needle is handed to me, both pieces, flat on your palm Image: a pinned seam approaching a presser foot, a hand pulling the nearest pin.
[bookmark: slide-6-the-first-seam]Slide 6: The first seam
· Edge on the quarter-inch guide
· Three or four reverse stitches at the start
· Slowest steady speed, hands to the sides, eyes just ahead of the needle
· Stop at the channel mark, reverse three or four, done Image: a seam being sewn with the reverse lever circled.
[bookmark: slide-7-day-1-close-count-and-close-down]Slide 7 (Day 1 close): Count and close down
· Pins counted, “N pins in work” in the notes column
· Presser foot down, power off, chair in
· Exit line: what does the reverse lever do, and where did you use it? Image: the count sheet’s notes column reading “6 pins in work.”
[bookmark: slide-8-day-2-do-now]Slide 8 (Day 2): Do now
· Needle down, foot up, pivot, foot down
· Where in today’s sewing will you actually use that? Image: the channel fold pinned around a bag top.
[bookmark: slide-9-threading-for-real-this-time]Slide 9: Threading, for real this time
· Licensed threaders: thread your machine from nothing, buddy verifies
· Not licensed yet: I thread yours, and we finish your license this week
· The manual at your machine is still the authority Image: the license line with two initials.
[bookmark: slide-10-the-channel]Slide 10: The channel
· Fold the top edge down one inch toward the wrong side, all the way around
· Pin every two inches, one pass at my iron
· Sew along the bottom of the fold
· BOTH ENDS STAY OPEN. Both ends stay open. Image: a channel seam circling a bag top with open gaps at both side seams, arrows pointing at the gaps.
[bookmark: slide-11-the-sampler-scrap]Slide 11: The sampler scrap
· Last four minutes: two scraps, one short seam, reverse-locked both ends
· Name on it in chalk
· This is Box 6 of your sampler card, sewn today so Thursday has time to score it Image: the sampler card’s Box 6, MACHINE SEAM.
[bookmark: X7485e886a40179d83021ed9f8b253e27912ebf4]Slide 12 (Day 2 close): Count and close down
· Count, notes column, close-down routine
· Exit card: how many seams done, and the one thing that gave you trouble Image: a row of machines, presser feet down.
[bookmark: slide-13-day-3-do-now]Slide 13 (Day 3): Do now
· What still has to happen for your bag to be finished, and how long will it take?
· List the six things that go on your sampler card Image: the six-box sampler card, empty.
[bookmark: slide-14-turn-cord-finish]Slide 14: Turn, cord, finish
· Turn through the top; corners out with an eraser or a chopstick, never the shears
· Safety pin on the cord, feed the channel, knot the ends, pull: it closes
· Trim every thread end; three hand stitches close any gap Image: a bag half turned right side out, and a safety pin leading a cord into a channel.
[bookmark: slide-15-the-five-point-self-check]Slide 15: The five-point self-check
· Cut to the pattern
· Seam on the line, both ends locked
· Even stitches
· Flat, not puckered
· Corners and ends closed Image: the checklist from Handout 05.11, Part 4.
[bookmark: slide-16-mount-the-sampler]Slide 16: Mount the sampler
· Six boxes: running stitch, backstitch, whipstitch, button, repair, machine seam
· Hand path: Box 6 is your best hand backstitch seam, labeled HAND PATH
· Label every box, run the self-check on each Image: a finished sampler card, six boxes filled.
[bookmark: slide-17-the-check-out-loud]Slide 17: The check, out loud
· Minute 20: machines closed down, tables cleared
· I score at your table, about 40 seconds each, out loud, so you hear the why
· The bag on the 20-point item rubric, the card on the 28-point check Image: the scoring grid from Assessment 05.2.
[bookmark: slide-18-day-3-close-the-reflection]Slide 18 (Day 3 close): The reflection
· Back of the card, three lines: best at, would redo, can now make or fix
· Three read aloud at the bell
· Cards to the FACS folder. Bags go home. You built that. Image: a hand pulling a drawstring bag closed.
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